Full modem wired and Full modem FOTA updates can be performed using the modem firmware in CBOR image
format, provided that you have the necessary support from the nRF Connect SDK and the device
hardware. The filename is as follows:
- mfw_nrf9151-ntn_1.0.0.cbor

Additionally, this release includes FOTA-TEST delta update images between the original firmware and
the FOTA-TEST image. The FOTA test update filenames are as follows:
- mfw_nrf9151-ntn_update_from_1.0.0_to_1.0.0-FOTA-TEST.bin
- mfw_nrf9151-ntn_update_from_1.0.0-FOTA-TEST_to_1.0.0.bin
- mfw_nrf9151-ntn_large_update_from_1.0.0_to_1.0.0-FOTA-TEST.bin
- mfw_nrf9151-ntn_large_update_from_1.0.0-FOTA-TEST_to_1.0.0.bin
 
UUID of mfw_nrf9151-ntn_1.0.0 is e95ba0f7-f555-4698-9d00-9d42205e375d
UUID of mfw_nrf9151-ntn_1.0.0-FOTA-TEST is baec6964-0826-46ef-b968-ce73c269521a